README FIRST - Flex Skimmer Bridge
=========================================

Start the program with:

  Start_FlexSkimmerBridge.bat

The batch file checks for the Microsoft .NET 8 Desktop Runtime. If it is missing, it opens the official Microsoft .NET 8 download page.

Install the Windows x64 Desktop Runtime, then run Start_FlexSkimmerBridge.bat again.

Main CW Skimmer requirements:

  Radio: SoftRock-IF
  Audio: DAX IQ 1 for Slice A
  CAT: SmartSDR CAT COM port for the target slice
  CAT RTS/DTR: Low
  Network/Telnet: enabled, port 7301, SKIMMER commands allowed

See Quick Start file or Manual for complete instructions.


